**TNT IP20 Indoor Logo Projector Technical Parameters**

|  |  |
| --- | --- |
| **Model：** | **TNT-QR-16** |
| 727324062fcc7889764c9a0b2e16cb5 | Wattage：16WLuminous Flux:2000LMGross Weight:1.5kgInner package size:32\*16\*14cmOuter package size:61\*51\*41cmQuantity of outer box:12pcs |
| **Input Voltage**:110V-240V Power adapter **/Working Frequency:**50-60HzLight Source Type：Big Power LED Lamp BeadAdaptor:Meanwell APC-16-350Color Temperature:7000K**Life Span:**40000hLamp Color:BlackShell Material: High-quality AluminumSurface Treatment:OxidationCooling Method:High efficient Cold forging heat dissipationWaterproof degree: IP20 indoor use onlyLight Spot Diameter:Project Distance multiply by 0.35Install Method:Embedded in ceilingRifice diameter:75mm |
|
|
|
|
|
|
|
|
|
| **Model：** | **TNT-GD-20** |
| 1595405044(1) | Wattage：20WLuminous Flux:2400LMGross Weight:1.5kgInner package size:39\*24\*14cmOuter package size:61\*51\*41cmQuantity of outer box:8pcs |
| **Input Voltage**:**100V-240V**Power adapter **/Working Frequency:**50-60HzLight Source Type：Big Power LED Lamp BeadAdaptor:Power gear 4cores trackColor Temperature:7000K**Life Span:**40000h **/** **Projection Angle：**360°Lamp Color:Black/white optionalShell Material: High-quality AluminumSurface Treatment:OxidationCooling Method:High efficient Cold forging heat dissipationWaterproof degree: IP20Light Spot Diameter:Project Distance multiply by 0.35Install Method:install in 4cores rail |

|  |  |
| --- | --- |
| **Model：** | TNT-SN-30R |
|  | Power：30WLuminous Flux:3600LMGross Weight:2kgInner package size:39\*24\*14cmOuter package size:61\*51\*41cmQuantity of outer box:8pcs |
| **Input Voltage**:**200V-240V**Power adapter **/Working Frequency:**50-60HzLight Source Type：Big Power LED Lamp BeadColor Temperature:7000KAdaptor：Meanwell APC35-700**Life Span:**40000h **/** **Projection Angle：**1080°Lamp Color:BlackShell Material: High-quality AluminumSurface Treatment:OxidationCooling Method:High efficient Cold forging heat dissipationWaterproof degree: IP20Light Spot Diameter:Project Distance multiply by 0.35Install Method:Surface mounted |